(footprint "RELAY_JC1A_PAN" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "JC1AF-DC12V-F ")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value RELAY_JC1A_PAN (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "*" (at -5.08 -13.110634) (layer F.SilkS))
  (fp_text user "*" (at -5.08 -13.110634) (layer F.Fab))
  (fp_text user "*" (at -5.08 -13.110634 unlocked) (layer "F.Fab"))
  (fp_text user "*" (at -5.08 -13.110634 unlocked) (layer "F.SilkS"))
  (pad "1" thru_hole circle (at -5.08 -11.4173) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask))
  (pad "3" thru_hole circle (at -5.08 11.4427) (size 2.413 2.413) (drill 1.905) (layers *.Cu *.Mask))
  (pad "5" thru_hole circle (at 5.08 3.8227) (size 2.413 2.413) (drill 1.905) (layers *.Cu *.Mask))
  (pad "6" thru_hole circle (at 5.08 -11.4173) (size 1.778 1.778) (drill 1.27) (layers *.Cu *.Mask))
)
