(footprint "RES_CMF50_VIS" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "CMF5010K000FKEB ")
  (attr through_hole)
  (fp_text reference "REF**" (at 4.191 0 unlocked) (layer F.SilkS))
  (fp_text value RES_CMF50_VIS (at 4.191 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 4.191 0 unlocked) (layer F.Fab))
  (pad "1" thru_hole rect (at 0 0) (size 1.2192 1.2192) (drill 0.7112) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at 8.382 0) (size 1.2192 1.2192) (drill 0.7112) (layers *.Cu *.Mask))
)
