(footprint "RHA0040R-IPC_A" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "THVD4431RHAR ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value RHA0040R-IPC_A (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "Designator781" (at -3.7338 -4.572 unlocked) (layer "F.SilkS"))
  (pad "1" smd rect (at -2.899999 -2.250001) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -2.899999 -1.749999) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -2.899999 -1.25) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -2.899999 -0.750001) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at -2.899999 -0.25) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at -2.899999 0.25) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at -2.899999 0.750001) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at -2.899999 1.25) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at -2.899999 1.749999) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd rect (at -2.899999 2.250001) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "11" smd rect (at -2.250001 2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "12" smd rect (at -1.749999 2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "13" smd rect (at -1.25 2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "14" smd rect (at -0.750001 2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "15" smd rect (at -0.25 2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "16" smd rect (at 0.25 2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "17" smd rect (at 0.750001 2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "18" smd rect (at 1.25 2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "19" smd rect (at 1.749999 2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "20" smd rect (at 2.250001 2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "21" smd rect (at 2.899999 2.250001) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "22" smd rect (at 2.899999 1.749999) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "23" smd rect (at 2.899999 1.25) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "24" smd rect (at 2.899999 0.750001) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "25" smd rect (at 2.899999 0.25) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "26" smd rect (at 2.899999 -0.25) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "27" smd rect (at 2.899999 -0.750001) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "28" smd rect (at 2.899999 -1.25) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "29" smd rect (at 2.899999 -1.749999) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "30" smd rect (at 2.899999 -2.250001) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "31" smd rect (at 2.250001 -2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "32" smd rect (at 1.749999 -2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "33" smd rect (at 1.25 -2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "34" smd rect (at 0.750001 -2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "35" smd rect (at 0.25 -2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "36" smd rect (at -0.25 -2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "37" smd rect (at -0.750001 -2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "38" smd rect (at -1.25 -2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "39" smd rect (at -1.749999 -2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "40" smd rect (at -2.250001 -2.899999 90) (size 0.599999 0.249999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "41" smd rect (at 0 0) (size 4.650001 4.650001) (layers "F.Cu" "F.Mask"))
  (pad "42" thru_hole circle (at 0 1.17) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "43" thru_hole circle (at 0.0254 0) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "44" thru_hole circle (at 0 -1.17) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "45" thru_hole circle (at -1.17 1.17) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "46" thru_hole circle (at -1.17 0) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "47" thru_hole circle (at -1.17 -1.17) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "48" thru_hole circle (at 1.17 1.17) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "49" thru_hole circle (at 1.17 0) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "50" thru_hole circle (at 1.17 -1.17) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "51" thru_hole circle (at 2.075 1.17) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "52" thru_hole circle (at 2.075 0) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "53" thru_hole circle (at 2.075 -1.17) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "54" thru_hole circle (at -2.075 1.17) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "55" thru_hole circle (at -2.075 0) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "56" thru_hole circle (at -2.075 -1.17) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "57" thru_hole circle (at -1.17 2.075) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "58" thru_hole circle (at 0 2.075) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "59" thru_hole circle (at 1.17 2.075) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "60" thru_hole circle (at -1.17 -2.075) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "61" thru_hole circle (at 0 -2.075) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "62" thru_hole circle (at 1.17 -2.075) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
)
