(module RPI-125 (layer F.Cu)
  (fp_text reference REF** (at 1.375 1) (layer F.SilkS))
  (fp_text value TRANS_RPI-125_ROM (at 1.375 1) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (pad 1 thru_hole circle (at 0 0) (size 0.9398 0.9398) (drill 0.4318) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 2.000001) (size 0.9398 0.9398) (drill 0.4318) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 2.750001 0) (size 0.9398 0.9398) (drill 0.4318) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 2.750001 2.000001) (size 0.9398 0.9398) (drill 0.4318) (layers *.Cu *.Mask))
)
