(module Resistor_SMD:R_2010_5025Metric (layer F.Cu) (tedit 63922815)
  (descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
  (tags resistor)
  (attr smd)
  (fp_text reference REF** (at 0 -2.28) (layer F.SilkS))
  (pad 2 smd roundrect (at 2.3125 0) (size 1.225 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.204082))
  (pad 1 smd roundrect (at -2.3125 0) (size 1.225 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.204082))
  (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2010_5025Metric.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
