(module R_Axial_DIN0614_L14.3mm_D5.7mm_P25.40mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
  (descr "Resistor, Axial_DIN0614 series, Axial, Horizontal, pin pitch=25.4mm, 1.5W, length*diameter=14.3*5.7mm^2")
  (tags "Resistor Axial_DIN0614 series Axial Horizontal pin pitch 25.4mm 1.5W length 14.3mm diameter 5.7mm")
  (fp_text reference REF** (at 12.7 -3.97) (layer F.SilkS))
  (fp_text value R_Axial_DIN0614_L14.3mm_D5.7mm_P25.40mm_Horizontal (at 12.7 3.97) (layer F.Fab))
  (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 25.4 0) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask))
  (fp_text user %R (at 12.7 0) (layer F.Fab))
  (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0614_L14.3mm_D5.7mm_P25.40mm_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)