(module R_Axial_DIN0617_L17.0mm_D6.0mm_P30.48mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
  (descr "Resistor, Axial_DIN0617 series, Axial, Horizontal, pin pitch=30.48mm, 2W, length*diameter=17*6mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
  (tags "Resistor Axial_DIN0617 series Axial Horizontal pin pitch 30.48mm 2W length 17mm diameter 6mm")
  (fp_text reference REF** (at 15.24 -4.12) (layer F.SilkS))
  (fp_text value R_Axial_DIN0617_L17.0mm_D6.0mm_P30.48mm_Horizontal (at 15.24 4.12) (layer F.Fab))
  (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 30.48 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask))
  (fp_text user %R (at 15.24 0) (layer F.Fab))
  (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0617_L17.0mm_D6.0mm_P30.48mm_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)