(module R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
  (descr "Resistor, Axial_DIN0918 series, Axial, Horizontal, pin pitch=22.86mm, 4W, length*diameter=18*9mm^2")
  (tags "Resistor Axial_DIN0918 series Axial Horizontal pin pitch 22.86mm 4W length 18mm diameter 9mm")
  (fp_text reference REF** (at 11.43 -5.62) (layer F.SilkS))
  (fp_text value R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal (at 11.43 5.62) (layer F.Fab))
  (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 22.86 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask))
  (fp_text user %R (at 11.43 0) (layer F.Fab))
  (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0918_L18.0mm_D9.0mm_P22.86mm_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)