(module SGP41-D-R4 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value DFN_SGP41-D-R4_SEN (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.032in/0.8mm" (at -4.2418 -0.40005) (layer Cmts.User))
  (fp_text user "0.016in/0.406mm" (at 4.2418 -0.8001) (layer Cmts.User))
  (fp_text user "0.094in/2.388mm" (at 0 -3.683) (layer Cmts.User))
  (fp_text user "0.03in/0.762mm" (at -1.1938 3.048) (layer Cmts.User))
  (fp_text user "0.069in/1.753mm" (at 3.683 0) (layer Cmts.User))
  (fp_text user "0.053in/1.346mm" (at 0 4.318) (layer Cmts.User))
  (pad 1 smd rect (at -1.1938 -0.8001) (size 0.762 0.4064) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.1938 0) (size 0.762 0.4064) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.1938 0.8001) (size 0.762 0.4064) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 1.1938 0.8001) (size 0.762 0.4064) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.1938 0) (size 0.762 0.4064) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.1938 -0.8001) (size 0.762 0.4064) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0 0) (size 1.3462 1.7526) (layers F.Cu F.Paste F.Mask))
)
