(module SHT40-AD1B-R2 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value SHT4x_SEN (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.031in/0.8mm" (at -3.7973 0) (layer Cmts.User))
  (fp_text user "0.012in/0.305mm" (at 3.7973 -0.4) (layer Cmts.User))
  (fp_text user "0.059in/1.499mm" (at 0 -3.2131) (layer Cmts.User))
  (fp_text user "0.028in/0.711mm" (at -0.7493 2.5781) (layer Cmts.User))
  (fp_text user "0.043in/1.092mm" (at 3.2131 0) (layer Cmts.User))
  (fp_text user "0.02in/0.508mm" (at 0 3.8481) (layer Cmts.User))
  (pad 1 smd rect (at -0.7493 -0.399999) (size 0.7112 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.7493 0.399999) (size 0.7112 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.7493 0.399999) (size 0.7112 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.7493 -0.399999) (size 0.7112 0.3048) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0 0) (size 0.508 1.0922) (layers F.Cu F.Paste F.Mask))
)
