(module SJ1-3523N (layer F.Cu) (tedit 63C59B08)
  (fp_text reference REF** (at 5.22 -2.99) (layer F.SilkS))
  (fp_text value " " (at -11.81 6.8) (layer F.SilkS))
  (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user * (at 0 0) (layer F.SilkS))
  (pad 4 thru_hole circle (at 5 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0 0 90) (size 2.008 1.308) (drill 0.0254) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0 5) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 10 5) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 0 7.5) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 10 7.5) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask))
  (pad 10 thru_hole oval (at 2.5 0 90) (size 2.008 1.308) (drill 0.0254) (layers *.Cu *.Mask))
  (pad 11 thru_hole oval (at 7.5 0 90) (size 2.008 1.308) (drill 0.0254) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 10 0 90) (size 2.008 1.308) (drill 0.0254) (layers *.Cu *.Mask))
  (pad 1 thru_hole oval (at 5 5) (size 2.008 1.308) (drill 0.0254) (layers *.Cu *.Mask))
)
