(module C_1825_4564Metric (layer F.Cu) (tedit 62D53811)
  (descr "Capacitor SMD 1825 (4564 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
  (tags capacitor)
  (attr smd)
  (fp_text reference REF** (at 0 -4.35) (layer F.SilkS))
  (fp_text value C_1825_4564Metric (at 0 4.35) (layer F.Fab))
  (pad 1 smd roundrect (at -2.05 0) (size 1.4 6.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.178571))
  (pad 2 smd roundrect (at 2.05 0) (size 1.4 6.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.178571))
  (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1825_4564Metric.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
