(module SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
  (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "SOIC SO")
  (attr smd)
  (fp_text reference REF** (at 0 -5.28) (layer F.SilkS))
  (fp_text value SOIC-14_3.9x8.7mm_P1.27mm (at 0 5.28) (layer F.Fab))
  (pad 1 smd rect (at -2.475 -3.81) (size 1.95 0.6) (layers F.Cu F.Mask F.Paste))
  (pad 2 smd rect (at -2.475 -2.54) (size 1.95 0.6) (layers F.Cu F.Mask F.Paste))
  (pad 3 smd rect (at -2.475 -1.27) (size 1.95 0.6) (layers F.Cu F.Mask F.Paste))
  (pad 4 smd rect (at -2.475 0) (size 1.95 0.6) (layers F.Cu F.Mask F.Paste))
  (pad 5 smd rect (at -2.475 1.27) (size 1.95 0.6) (layers F.Cu F.Mask F.Paste))
  (pad 6 smd rect (at -2.475 2.54) (size 1.95 0.6) (layers F.Cu F.Mask F.Paste))
  (pad 7 smd rect (at -2.475 3.81) (size 1.95 0.6) (layers F.Cu F.Mask F.Paste))
  (pad 8 smd rect (at 2.475 3.81) (size 1.95 0.6) (layers F.Cu F.Mask F.Paste))
  (pad 9 smd rect (at 2.475 2.54) (size 1.95 0.6) (layers F.Cu F.Mask F.Paste))
  (pad 10 smd rect (at 2.475 1.27) (size 1.95 0.6) (layers F.Cu F.Mask F.Paste))
  (pad 11 smd rect (at 2.475 0) (size 1.95 0.6) (layers F.Cu F.Mask F.Paste))
  (pad 12 smd rect (at 2.475 -1.27) (size 1.95 0.6) (layers F.Cu F.Mask F.Paste))
  (pad 13 smd rect (at 2.475 -2.54) (size 1.95 0.6) (layers F.Cu F.Mask F.Paste))
  (pad 14 smd rect (at 2.475 -3.81) (size 1.95 0.6) (layers F.Cu F.Mask F.Paste))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)