(module Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm (layer F.Cu) (tedit 61B055C5)
  (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "SOIC SO")
  (attr smd)
  (fp_text reference REF** (at 0 -7.35) (layer F.SilkS))
  (fp_text value SOIC-20W_7.5x12.8mm_P1.27mm (at 0 7.35) (layer F.Fab))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (pad 20 smd rect (at 4.65 -5.715) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at 4.65 -4.445) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 4.65 -3.175) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at 4.65 -1.905) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 4.65 -0.635) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 4.65 0.635) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 4.65 1.905) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 4.65 3.175) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 4.65 4.445) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 4.65 5.715) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -4.65 5.715) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -4.65 4.445) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -4.65 3.175) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -4.65 1.905) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -4.65 0.635) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -4.65 -0.635) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -4.65 -1.905) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -4.65 -3.175) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -4.65 -4.445) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -4.65 -5.715) (size 2.05 0.6) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
