(footprint "_09 Lib_PROJECTS_Infineon_Task Tracker Parts_Conversion_INP_NPI Conversion_2024_NPI Conversion_January-24_Working_Set-1_IAUCN04S6N007T_Altium_SOP100P768X144-10N-V.PcbLib_SOP100P768X144-10N-V" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (fp_text reference "Designator" (at -5.45 -3.125 unlocked) (layer "F.SilkS"))
  (fp_text value "Comment" (at 0 0 unlocked) (layer "F.Fab") hide)
  (fp_text user "${REFERENCE}" (at -2.875 0.3 unlocked) (layer "F.Fab"))
  (pad "1" smd rect (at -3.73 -2) (size 1.75 0.52) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "2" smd rect (at -3.73 -1) (size 1.75 0.52) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "3" smd rect (at -3.73 0) (size 1.75 0.52) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "4" smd rect (at -3.73 1) (size 1.75 0.52) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "5" smd rect (at -3.73 2) (size 1.75 0.52) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "6" smd rect (at 3.73 2) (size 1.75 0.52) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "7" smd rect (at 3.73 1) (size 1.75 0.52) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "8" smd rect (at 3.73 0) (size 1.75 0.52) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "9" smd rect (at 3.73 -1) (size 1.75 0.52) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "10" smd rect (at 3.73 -2) (size 1.75 0.52) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/PG-LHDSO-10-3_Z8B00220316_V04_3D.stp"
    (offset (xyz 0 -0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -0 -0 0))
  )
)
