(footprint "SOP2_8PIN_208MIL_MRN" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "MT25QL128ABA1ESE-0SIT ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value SOP2_8PIN_208MIL_MRN (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "*" (at -3.9497 -3.5814) (layer F.SilkS))
  (fp_text user "*" (at -2.3622 -2.667) (layer F.Fab))
  (fp_text user "*" (at -3.9497 -3.5814 unlocked) (layer "F.SilkS"))
  (fp_text user "*" (at -2.3622 -2.667 unlocked) (layer "F.Fab"))
  (pad "1" smd rect (at -3.6957 -1.905) (size 1.8288 0.5334) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -3.6957 -0.635) (size 1.8288 0.5334) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -3.6957 0.635) (size 1.8288 0.5334) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -3.6957 1.905) (size 1.8288 0.5334) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at 3.6957 1.905) (size 1.8288 0.5334) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at 3.6957 0.635) (size 1.8288 0.5334) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at 3.6957 -0.635) (size 1.8288 0.5334) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at 3.6957 -1.905) (size 1.8288 0.5334) (layers "F.Cu" "F.Paste" "F.Mask"))
)
