(footprint "SOT-1220UDFN6B_TOS" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "SSM6K518NU_LF ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value SOT-1220UDFN6B_TOS (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (pad "1" smd rect (at -1.0668 -0.649999) (size 0.5842 0.254) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -1.0668 0) (size 0.5842 0.254) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -1.0668 0.649999) (size 0.5842 0.254) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at 1.0668 0.649999) (size 0.5842 0.254) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at 1.0668 0) (size 0.5842 0.254) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at 1.0668 -0.649999) (size 0.5842 0.254) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at 0 -0.325) (size 1.143 0.9398) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at 0 0.65) (size 0.762 0.3048) (layers "F.Cu" "F.Paste" "F.Mask"))
)
