(module SRR1260-1R0Y (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value IND_BOURNS_SRR1260 (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.213in/5.41mm" (at 5.7531 0) (layer Cmts.User))
  (fp_text user "0.496in/12.598mm" (at 0 9.4488) (layer Cmts.User))
  (fp_text user "0.268in/6.807mm" (at 0 -9.4488) (layer Cmts.User))
  (pad 1 smd rect (at -4.8514 0) (size 2.8956 5.4102) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 4.8514 0) (size 2.8956 5.4102) (layers F.Cu F.Paste F.Mask))
)
