(module SSM6N15AFU_LF (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value SOT-363   US6_TOS (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.026in/0.65mm" (at -4.0894 -0.325) (layer Cmts.User))
  (fp_text user "0.014in/0.356mm" (at 4.0894 -0.65) (layer Cmts.User))
  (fp_text user "0.082in/2.083mm" (at 0 -3.4163) (layer Cmts.User))
  (fp_text user "0.033in/0.838mm" (at -1.0414 3.4163) (layer Cmts.User))
  (fp_text user "*" (at -1.2954 -2.1486) (layer F.SilkS))
  (fp_text user "*" (at -0.2413 -0.9271) (layer F.Fab))
  (pad 1 smd rect (at -1.0414 -0.649999) (size 0.8382 0.3556) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.0414 0) (size 0.8382 0.3556) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.0414 0.649999) (size 0.8382 0.3556) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 1.0414 0.649999) (size 0.8382 0.3556) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.0414 0) (size 0.8382 0.3556) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.0414 -0.649999) (size 0.8382 0.3556) (layers F.Cu F.Paste F.Mask))
)
