(module SSOP-20_5.3x7.2mm_P0.65mm (layer F.Cu) (tedit 5D9F72B1)
  (descr "SSOP, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/40001800C.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "SSOP SO")
  (attr smd)
  (fp_text reference REF** (at 0 -4.55) (layer F.SilkS))
  (fp_text value SSOP-20_5.3x7.2mm_P0.65mm (at 0 4.55) (layer F.Fab))
  (pad 1 smd rect (at -3.5 -2.925) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 2 smd rect (at -3.5 -2.275) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 3 smd rect (at -3.5 -1.625) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 4 smd rect (at -3.5 -0.975) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 5 smd rect (at -3.5 -0.325) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 6 smd rect (at -3.5 0.325) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 7 smd rect (at -3.5 0.975) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 8 smd rect (at -3.5 1.625) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 9 smd rect (at -3.5 2.275) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 10 smd rect (at -3.5 2.925) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 11 smd rect (at 3.5 2.925) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 12 smd rect (at 3.5 2.275) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 13 smd rect (at 3.5 1.625) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 14 smd rect (at 3.5 0.975) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 15 smd rect (at 3.5 0.325) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 16 smd rect (at 3.5 -0.325) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 17 smd rect (at 3.5 -0.975) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 18 smd rect (at 3.5 -1.625) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 19 smd rect (at 3.5 -2.275) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (pad 20 smd rect (at 3.5 -2.925) (size 1.9 0.5) (layers F.Cu F.Mask F.Paste))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-20_5.3x7.2mm_P0.65mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)