(footprint "SSOP-24_5.3x8.2mm_P0.65mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "24-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
	(tags "SSOP 0.65")
	(property "Reference" "REF**"
		(at 0 -5.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "SSOP-24_5.3x8.2mm_P0.65mm"
		(at 0 5.25 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.6 -3.575)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "2" smd rect
		(at -3.6 -2.925)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at -3.6 -2.275)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "4" smd rect
		(at -3.6 -1.625)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "5" smd rect
		(at -3.6 -0.975)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "6" smd rect
		(at -3.6 -0.325)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "7" smd rect
		(at -3.6 0.325)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "8" smd rect
		(at -3.6 0.975)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "9" smd rect
		(at -3.6 1.625)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "10" smd rect
		(at -3.6 2.275)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "11" smd rect
		(at -3.6 2.925)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "12" smd rect
		(at -3.6 3.575)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "13" smd rect
		(at 3.6 3.575)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "14" smd rect
		(at 3.6 2.925)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "15" smd rect
		(at 3.6 2.275)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "16" smd rect
		(at 3.6 1.625)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "17" smd rect
		(at 3.6 0.975)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "18" smd rect
		(at 3.6 0.325)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "19" smd rect
		(at 3.6 -0.325)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "20" smd rect
		(at 3.6 -0.975)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "21" smd rect
		(at 3.6 -1.625)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "22" smd rect
		(at 3.6 -2.275)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "23" smd rect
		(at 3.6 -2.925)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "24" smd rect
		(at 3.6 -3.575)
		(size 1.75 0.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-24_5.3x8.2mm_P0.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)