(footprint "STGAP2HDMTR" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (descr " SSOP 32 LEAD 300 MIL PKG .0315  P ")
  (tags "Integrated Circuit")
  (attr smd)
  (fp_text reference "IC**" (at 0 0) (layer "F.SilkS"))
  (fp_text value "STGAP2HDMTR" (at 0 0) (layer "F.SilkS") hide)
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
  (pad "1" smd rect (at -4.8 -6.8 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -4.8 -6 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -4.8 -5.2 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -4.8 -4.4 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at -4.8 -3.6 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at -4.8 -2.8 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at -4.8 -2 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at -4.8 -1.2 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at -4.8 -0.4 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd rect (at -4.8 0.4 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "11" smd rect (at -4.8 1.2 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "12" smd rect (at -4.8 2 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "13" smd rect (at -4.8 2.8 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "14" smd rect (at -4.8 3.6 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "15" smd rect (at -4.8 4.4 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "16" smd rect (at -4.8 5.2 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "17" smd rect (at -4.8 6 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "18" smd rect (at -4.8 6.8 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "19" smd rect (at 4.8 6.8 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "20" smd rect (at 4.8 6 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "21" smd rect (at 4.8 5.2 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "22" smd rect (at 4.8 4.4 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "23" smd rect (at 4.8 3.6 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "24" smd rect (at 4.8 2.8 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "25" smd rect (at 4.8 2 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "30" smd rect (at 4.8 -2 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "31" smd rect (at 4.8 -2.8 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "32" smd rect (at 4.8 -3.6 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "33" smd rect (at 4.8 -4.4 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "34" smd rect (at 4.8 -5.2 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "35" smd rect (at 4.8 -6 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "36" smd rect (at 4.8 -6.8 90) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask"))
)
