(module STGE200NB60S (layer F.Cu)
  (fp_text reference REF** (at -7.493 6.35) (layer F.SilkS))
  (fp_text value ISOTOP_STM (at -7.493 6.35) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at -27.432 12.7) (layer F.Fab))
  (fp_text user "*" (at -27.432 12.7) (layer F.SilkS))
  (pad 1 thru_hole circle (at -14.986 12.7) (size 4.699 4.699) (drill 4.191) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 12.7) (size 4.699 4.699) (drill 4.191) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -14.986 0) (size 4.699 4.699) (drill 4.191) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 0) (size 4.699 4.699) (drill 4.191) (layers *.Cu *.Mask))
  (pad 7 np_thru_hole circle (at -29.972 6.35) (size 4.8006 4.8006) (drill 4.2926) (layers))
  (pad 8 np_thru_hole circle (at 14.986 6.35) (size 4.8006 4.8006) (drill 4.2926) (layers))
)
