(footprint "ST_MultiPowerSO-30"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "MultiPowerSO-30 3EP 16.0x17.2mm Pitch 1mm (http://www.st.com/resource/en/datasheet/vnh2sp30-e.pdf)")
	(tags "MultiPowerSO-30 3EP 16.0x17.2mm Pitch 1mm")
	(property "Reference" "REF**"
		(at 0 -9.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "ST_MultiPowerSO-30"
		(at 0 9.6 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -9.125 -7 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "2" smd rect
		(at -9.125 -6 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at -9.125 -5 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "4" smd rect
		(at -9.125 -4 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "5" smd rect
		(at -9.125 -3 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "6" smd rect
		(at -9.125 -2 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "7" smd rect
		(at -9.125 -1 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "8" smd rect
		(at -9.125 0 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "9" smd rect
		(at -9.125 1 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "10" smd rect
		(at -9.125 2 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "11" smd rect
		(at -9.125 3 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "12" smd rect
		(at -9.125 4 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "13" smd rect
		(at -9.125 5 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "14" smd rect
		(at -9.125 6 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "15" smd rect
		(at -9.125 7 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "16" smd rect
		(at 9.125 7 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "17" smd rect
		(at 9.125 6 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "18" smd rect
		(at 9.125 5 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "19" smd rect
		(at 9.125 4 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "20" smd rect
		(at 9.125 3 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "21" smd rect
		(at 9.125 2 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "22" smd rect
		(at 9.125 1 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "23" smd rect
		(at 9.125 0 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "24" smd rect
		(at 9.125 -1 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "25" smd rect
		(at 9.125 -2 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "26" smd rect
		(at 9.125 -3 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "27" smd rect
		(at 9.125 -4 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "28" smd rect
		(at 9.125 -5 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "29" smd rect
		(at 9.125 -6 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "30" smd rect
		(at 9.125 -7 270)
		(size 0.66 1.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "31" smd rect
		(at -3.05 0)
		(size 5.25 10.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "32" smd rect
		(at 3.05 4.165)
		(size 5.25 6.23)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "33" smd rect
		(at 3.05 -4.165)
		(size 5.25 6.23)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/ST_MultiPowerSO-30.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)