(footprint "SW_Kailh_Choc_V1_THT" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Kailh Choc V1 (PG1350) low profile mechanical keyboard switch, through-hole soldering, single-sided mounting.")
  (tags "switch, low_profile")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -8.5 unlocked) (layer "F.SilkS") hide)
  (pad "" np_thru_hole circle (at -5.5 0) (size 1.7018 1.7018) (drill 1.7018) (layers "*.Cu" "*.Mask"))
  (pad "" np_thru_hole circle (at 0 0) (size 3.429 3.429) (drill 3.429) (layers "*.Cu" "*.Mask"))
  (pad "" np_thru_hole circle (at 5.5 0) (size 1.7018 1.7018) (drill 1.7018) (layers "*.Cu" "*.Mask"))
  (pad "1" thru_hole circle (at 0 5.9) (size 2 2) (drill 1.27) (layers "*.Cu" "B.Mask"))
  (pad "2" thru_hole circle (at -5 3.8) (size 2 2) (drill 1.27) (layers "*.Cu" "B.Mask"))
)
