(module SW_SPST_Omron_B3FS-105xP (layer F.Cu) (tedit 5E6E8EEE)
  (descr "Surface Mount Tactile Switch for High-Density Mounting, 7.3mm height, https://omronfs.omron.com/en_US/ecb/products/pdf/en-b3fs.pdf")
  (tags "Tactile Switch")
  (attr smd)
  (fp_text reference REF** (at 0 -4.3) (layer F.SilkS))
  (fp_text value SW_SPST_Omron_B3FS-105xP (at 0 4.2) (layer F.Fab))
  (fp_text user %R (at 0 -2.2) (layer F.Fab))
  (pad 1 smd rect (at -4 -2.25 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 4 -2.25 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -4 2.25 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 4 2.25 180) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_Omron_B3FS-105xP.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
