(module Button_Switch_SMD:SW_SPST_TL3342 (layer F.Cu) (tedit 631B184A)
  (descr "Low-profile SMD Tactile Switch, https://www.e-switch.com/system/asset/product_line/data_sheet/165/TL3342.pdf")
  (tags "SPST Tactile Switch")
  (attr smd)
  (fp_text reference REF** (at 0 -3.75) (layer F.SilkS))
  (fp_text value SW_SPST_TL3342 (at 0 3.75) (layer F.Fab))
  (fp_text user %R (at 0 -3.75) (layer F.Fab))
  (pad P smd rect (at 3.15 1.9) (size 1.7 1) (layers F.Cu F.Paste F.Mask))
  (pad P1 smd rect (at -3.15 1.9) (size 1.7 1) (layers F.Cu F.Paste F.Mask))
  (pad S smd rect (at 3.15 -1.9) (size 1.7 1) (layers F.Cu F.Paste F.Mask))
  (pad S1 smd rect (at -3.15 -1.9) (size 1.7 1) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_TL3342.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
