(module Sensirion_DFN-8-1EP_2.5x2.5mm_P0.5mm_EP1.1x1.7mm (layer F.Cu) (tedit 5F15CF57)
  (descr "Sensirion DFN-8 SHT3x-DIS (https://www.sensirion.com/fileadmin/user_upload/customers/sensirion/Dokumente/2_Humidity_Sensors/Datasheets/Sensirion_Humidity_Sensors_SHT3x_Datasheet_digital.pdf)")
  (tags "sensirion dfn nolead")
  (attr smd)
  (fp_text reference REF** (at 0 -2.25) (layer F.SilkS))
  (fp_text value Sensirion_DFN-8-1EP_2.5x2.5mm_P0.5mm_EP1.1x1.7mm (at 0 2.5) (layer F.Fab))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (pad "" smd custom (at 0 0) (size 0.9 0.9) (layers F.Paste)
    (zone_connect 0)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly (pts
         (xy 0.45 0.8) (xy -0.45 0.8) (xy -0.45 -0.53) (xy -0.18 -0.8) (xy 0.45 -0.8)
) (width 0))
    ))
  (pad 9 smd custom (at 0 0) (size 1 1) (layers F.Cu F.Mask)
    (zone_connect 0)
    (options (clearance outline) (anchor circle))
    (primitives
      (gr_poly (pts
         (xy 0.5 0.85) (xy -0.5 0.85) (xy -0.5 -0.55) (xy -0.2 -0.85) (xy 0.5 -0.85)
) (width 0))
    ))
  (pad 8 smd rect (at 1.175 -0.75) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.175 -0.25) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.175 0.25) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.175 0.75) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.175 0.75 180) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.175 0.25) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.175 -0.25) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -1.175 -0.75) (size 0.55 0.25) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Sensor_Humidity.3dshapes/Sensirion_DFN-8-1EP_2.5x2.5mm_P0.5mm_EP1.1x1.7mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
