(module Jumper:SolderJumper-3_P1.3mm_Bridged12_Pad1.0x1.5mm (layer F.Cu) (tedit 628E7A02)
  (descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
  (tags "solder jumper open")
  (attr virtual)
  (fp_text reference REF** (at 0 -1.8) (layer F.SilkS))
  (fp_text value SolderJumper-3_P1.3mm_Bridged12_Pad1.0x1.5mm (at 0 2) (layer F.Fab))
  (pad 13 smd rect (at -0.508 0) (size 1 0.6) (layers F.Cu F.Mask))
  (pad 2 smd rect (at 0 0) (size 1 1.5) (layers F.Cu F.Mask))
  (pad 3 smd rect (at 1.3 0) (size 1 1.5) (layers F.Cu F.Mask))
  (pad 1 smd rect (at -1.3 0) (size 1 1.5) (layers F.Cu F.Mask))
)
