(module TC647BEUATR (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value MSOP8_MC_MCH (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.026in/0.65mm" (at -5.0927 -0.65) (layer Cmts.User))
  (fp_text user "0.018in/0.457mm" (at 5.0927 -0.975) (layer Cmts.User))
  (fp_text user "0.161in/4.089mm" (at 0 -3.9116) (layer Cmts.User))
  (fp_text user "0.06in/1.524mm" (at -2.0447 3.9116) (layer Cmts.User))
  (fp_text user "*" (at -2.2987 -2.5752) (layer F.SilkS))
  (fp_text user "*" (at -1.1176 -1.4224) (layer F.Fab))
  (pad 1 smd rect (at -2.0447 -0.974999) (size 1.524 0.4572) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.0447 -0.325001) (size 1.524 0.4572) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.0447 0.325001) (size 1.524 0.4572) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.0447 0.974999) (size 1.524 0.4572) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 2.0447 0.974999) (size 1.524 0.4572) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2.0447 0.325001) (size 1.524 0.4572) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 2.0447 -0.325001) (size 1.524 0.4572) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 2.0447 -0.974999) (size 1.524 0.4572) (layers F.Cu F.Paste F.Mask))
)
