(module TC78B016FTG_EL (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value P-WQFN36-0505-0p50-001_TOS (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at -4.430401 -1.75) (layer Cmts.User))
  (fp_text user "0.028in/0.705mm" (at -2.452401 -5.5004) (layer Cmts.User))
  (fp_text user "0.008in/0.199mm" (at -5.5004 2.452401) (layer Cmts.User))
  (fp_text user "0.193in/4.905mm" (at 0 8.040401) (layer Cmts.User))
  (fp_text user "0.193in/4.905mm" (at 8.040401 0.635) (layer Cmts.User))
  (fp_text user "0.142in/3.6mm" (at 0 4.848) (layer Cmts.User))
  (fp_text user "0.142in/3.6mm" (at 4.848 -0.635) (layer Cmts.User))
  (fp_text user "*" (at -3.439801 -2.25) (layer F.SilkS))
  (fp_text user "*" (at -2.100001 -2.25) (layer F.Fab))
  (pad 1 smd rect (at -2.5024 -2.000001 90) (size 0.1992 0.6048) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.4524 -1.5 90) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.4524 -1.000001 90) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.4524 -0.499999 90) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -2.4524 0 90) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -2.4524 0.499999 90) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -2.4524 1.000001 90) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -2.4524 1.5 90) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -2.5024 2.000001 90) (size 0.1992 0.6048) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -2.000001 2.5024) (size 0.1992 0.6048) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -1.5 2.4524) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -1.000001 2.4524) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -0.499999 2.4524) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 0 2.4524) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 0.499999 2.4524) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 1.000001 2.4524) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at 1.5 2.4524) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 2.000001 2.5024) (size 0.1992 0.6048) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at 2.5024 2.000001 90) (size 0.1992 0.6048) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 2.4524 1.5 90) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 2.4524 1.000001 90) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 2.4524 0.499999 90) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 2.4524 0 90) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 2.4524 -0.499999 90) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 2.4524 -1.000001 90) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at 2.4524 -1.5 90) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at 2.5024 -2.000001 90) (size 0.1992 0.6048) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at 2.000001 -2.5024) (size 0.1992 0.6048) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at 1.5 -2.4524) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd rect (at 1.000001 -2.4524) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 31 smd rect (at 0.499999 -2.4524) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 32 smd rect (at 0 -2.4524) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 33 smd rect (at -0.499999 -2.4524) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 34 smd rect (at -1.000001 -2.4524) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 35 smd rect (at -1.5 -2.4524) (size 0.1992 0.7048) (layers F.Cu F.Paste F.Mask))
  (pad 36 smd rect (at -2.000001 -2.5024) (size 0.1992 0.6048) (layers F.Cu F.Paste F.Mask))
  (pad 37 smd rect (at 0 0) (size 3.6 3.6) (layers F.Cu F.Paste F.Mask))
)
