(footprint "TDSON-8-1"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Power MOSFET package, TDSON-8-1, 5.15x5.9mm (https://www.infineon.com/cms/en/product/packages/PG-TDSON/PG-TDSON-8-1/)")
	(tags "tdson ")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "TDSON-8-1"
		(at 0 3.5 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd roundrect
		(at -2.9 -1.905)
		(size 0.85 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.05)
	)
	(pad "2" smd roundrect
		(at -2.9 -0.635)
		(size 0.85 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.05)
	)
	(pad "3" smd roundrect
		(at -2.9 0.635)
		(size 0.85 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.05)
	)
	(pad "4" smd roundrect
		(at -2.9 1.905)
		(size 0.85 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.05)
	)
	(pad "5" smd rect
		(at 1.05 0)
		(size 4.55 4.41)
		(layers "F.Cu")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TDSON-8-1.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)