(module TFTSPI_2_8_240x320_TOUCH (layer F.Cu) (tedit 601BFEDB)
  (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x14 2.54mm single row")
  (fp_text reference LCD1 (at 0 -2.33) (layer F.SilkS) hide)
  (fp_text value LCD (at 0 5) (layer F.Fab))
  (fp_text user %R (at 0 9 180) (layer F.Fab))
  (fp_text user VCC (at 37.75 16.75) (layer F.SilkS))
  (fp_text user GND (at 37.75 14) (layer F.SilkS))
  (fp_text user CS (at 38.25 11.5) (layer F.SilkS))
  (fp_text user RESET (at 37 9) (layer F.SilkS))
  (fp_text user DC (at 38.25 6.5) (layer F.SilkS))
  (fp_text user MOSI (at 37.5 3.75) (layer F.SilkS))
  (fp_text user SCK (at 37.75 1.25) (layer F.SilkS))
  (fp_text user LED (at 38 -1.25) (layer F.SilkS))
  (fp_text user MISO (at 37.5 -3.75) (layer F.SilkS))
  (fp_text user T_CLK (at 37 -6.25) (layer F.SilkS))
  (fp_text user T_CS (at 37.5 -8.75) (layer F.SilkS))
  (fp_text user T_DIN (at 37.25 -11.25) (layer F.SilkS))
  (fp_text user T_DO (at 37.5 -13.75) (layer F.SilkS))
  (fp_text user T_IRQ (at 37.25 -16.5) (layer F.SilkS))
  (fp_text user SD_CS (at -36.4 4.35) (layer F.SilkS))
  (fp_text user SD_MOSI (at -35.566667 1.6) (layer F.SilkS))
  (fp_text user SD_MISO (at -35.566667 -0.9) (layer F.SilkS))
  (fp_text user SD_SCK (at -35.9 -3.4) (layer F.SilkS))
  (fp_text user "SD CARD" (at -4 27) (layer F.SilkS))
  (pad 1 thru_hole rect (at 41 -16.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 41 -13.96) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 41 -11.42) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 41 -8.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 41 -6.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 41 -3.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 7 thru_hole oval (at 41 -1.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 8 thru_hole oval (at 41 1.28) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 9 thru_hole oval (at 41 3.82) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 10 thru_hole oval (at 41 6.36) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 11 thru_hole oval (at 41 8.9) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 12 thru_hole oval (at 41 11.44) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 13 thru_hole oval (at 41 13.98) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 14 thru_hole oval (at 41 16.52) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad SD1 thru_hole oval (at -40.5 -3.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad SD4 thru_hole oval (at -40.5 4.12) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad SD3 thru_hole oval (at -40.5 1.58) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad SD2 thru_hole oval (at -40.5 -0.96) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 36 -22) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 36 22) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -40 -22) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -40 22) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x14_Pitch2.54mm.wrl
    (offset (xyz 41 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
  (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
    (offset (xyz -41 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 -90))
  )
  (model ${KISYS3DMOD}/Display.3dshapes/CR2013-MI2120.wrl
    (offset (xyz 41 -13 7.5))
    (scale (xyz 1.26 1.22 1))
    (rotate (xyz 0 0 180))
  )
)
