(module D_DO-34_SOD68_P12.70mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
  (descr "Diode, DO-34_SOD68 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf")
  (tags "Diode DO-34_SOD68 series Axial Horizontal pin pitch 12.7mm  length 3.04mm diameter 1.6mm")
  (fp_text reference REF** (at 6.35 -1.92) (layer F.SilkS))
  (fp_text value D_DO-34_SOD68_P12.70mm_Horizontal (at 6.35 1.92) (layer F.Fab))
  (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.75) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 12.7 0) (size 1.5 1.5) (drill 0.75) (layers *.Cu *.Mask))
  (fp_text user %R (at 6.578 0) (layer F.Fab))
  (fp_text user K (at 0 -1.75) (layer F.Fab))
  (fp_text user K (at 0 -1.75) (layer F.SilkS))
  (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-34_SOD68_P12.70mm_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)