(module D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp (layer F.Cu) (tedit 5AE50CD5)
  (descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
  (tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
  (fp_text reference REF** (at 1.27 -2.326371) (layer F.SilkS))
  (fp_text value D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp (at 1.27 3.215371) (layer F.Fab))
  (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (fp_text user %R (at 1.27 -2.326371) (layer F.Fab))
  (fp_text user A (at 4.34 0) (layer F.Fab))
  (fp_text user A (at 4.34 0) (layer F.SilkS))
  (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)