(module D_DO-41_SOD81_P5.08mm_Vertical_KathodeUp (layer F.Cu) (tedit 5AE50CD5)
  (descr "Diode, DO-41_SOD81 series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
  (tags "Diode DO-41_SOD81 series Axial Vertical pin pitch 5.08mm  length 5.2mm diameter 2.7mm")
  (fp_text reference REF** (at 2.54 -2.750635) (layer F.SilkS))
  (fp_text value D_DO-41_SOD81_P5.08mm_Vertical_KathodeUp (at 2.54 2.750635) (layer F.Fab))
  (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 5.08 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask))
  (fp_text user %R (at 2.54 -2.750635) (layer F.Fab))
  (fp_text user K (at 1.8 1.1) (layer F.Fab))
  (fp_text user K (at 1.8 1.1) (layer F.SilkS))
  (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P5.08mm_Vertical_KathodeUp.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)