(footprint "TI_SO-PowerPAD-8"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "8-Lead Plastic PSOP, Exposed Die Pad (TI DDA0008B, see http://www.ti.com/lit/ds/symlink/lm3404.pdf)")
	(tags "SSOP 0.50 exposed pad")
	(property "Reference" "REF**"
		(at 0 -3.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "TI_SO-PowerPAD-8"
		(at 0 3.4 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(clearance 0.2)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.78 -1.905)
		(size 1.91 0.61)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "2" smd rect
		(at -2.78 -0.635)
		(size 1.91 0.61)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at -2.78 0.635)
		(size 1.91 0.61)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "4" smd rect
		(at -2.78 1.905)
		(size 1.91 0.61)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "5" smd rect
		(at 2.78 1.905)
		(size 1.91 0.61)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "6" smd rect
		(at 2.78 0.635)
		(size 1.91 0.61)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "7" smd rect
		(at 2.78 -0.635)
		(size 1.91 0.61)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "8" smd rect
		(at 2.78 -1.905)
		(size 1.91 0.61)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "9" smd rect
		(at -0.6025 -0.775)
		(size 1.205 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "9" smd rect
		(at -0.6025 0.775)
		(size 1.205 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "9" smd rect
		(at 0.6025 -0.775)
		(size 1.205 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_paste_margin_ratio -0.2)
	)
	(pad "9" smd rect
		(at 0.6025 0.775)
		(size 1.205 1.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_paste_margin_ratio -0.2)
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TI_SO-PowerPAD-8.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)