(module TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical (layer F.Cu) (tedit 5AF05A31)
  (descr "TO-220-11, Vertical, RM 1.7mm, staggered type-1, see http://www.st.com/resource/en/datasheet/tda7391lv.pdf")
  (tags "TO-220-11 Vertical RM 1.7mm staggered type-1")
  (fp_text reference REF** (at 8.5 -10.7) (layer F.SilkS))
  (fp_text value TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical (at 8.5 2.15) (layer F.Fab))
  (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 1.7 -5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 3.4 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 5.1 -5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 6.8 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 8.5 -5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 7 thru_hole oval (at 10.2 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 8 thru_hole oval (at 11.9 -5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 9 thru_hole oval (at 13.6 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 10 thru_hole oval (at 15.3 -5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 11 thru_hole oval (at 17 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (fp_text user %R (at 8.5 -10.7) (layer F.Fab))
  (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-11_P3.4x5.08mm_StaggerOdd_Lead4.85mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)