(module TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical (layer F.Cu) (tedit 5AF05A31)
  (descr "TO-220-15, Vertical, RM 1.27mm, staggered type-1, see http://www.st.com/resource/en/datasheet/l298.pdf")
  (tags "TO-220-15 Vertical RM 1.27mm staggered type-1")
  (fp_text reference REF** (at 8.89 -10.7) (layer F.SilkS))
  (fp_text value TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical (at 8.89 2.15) (layer F.Fab))
  (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 1.27 -5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 3.81 -5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 6.35 -5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 7 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 8 thru_hole oval (at 8.89 -5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 9 thru_hole oval (at 10.16 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 10 thru_hole oval (at 11.43 -5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 11 thru_hole oval (at 12.7 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 12 thru_hole oval (at 13.97 -5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 13 thru_hole oval (at 15.24 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 14 thru_hole oval (at 16.51 -5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 15 thru_hole oval (at 17.78 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (fp_text user %R (at 8.89 -10.7) (layer F.Fab))
  (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-15_P2.54x2.54mm_StaggerOdd_Lead4.58mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)