(module TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical (layer F.Cu) (tedit 5AF05A31)
  (descr "TO-220-5, Vertical, RM 1.7mm, Pentawatt, Multiwatt-5, staggered type-1, see http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-to-220/to-220_5_05-08-1421.pdf?domain=www.linear.com, https://www.diodes.com/assets/Package-Files/TO220-5.pdf")
  (tags "TO-220-5 Vertical RM 1.7mm Pentawatt Multiwatt-5 staggered type-1")
  (fp_text reference REF** (at 3.4 -9.32) (layer F.SilkS))
  (fp_text value TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical (at 3.4 2.15) (layer F.Fab))
  (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 1.7 -3.7) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 3.4 0) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 5.1 -3.7) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 6.8 0) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
  (fp_text user %R (at 3.4 -9.32) (layer F.Fab))
  (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)