(footprint "TO-220AB_STM" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "ACST610-8T ")
  (attr through_hole)
  (fp_text reference "REF**" (at 2.54 -0.65 unlocked) (layer F.SilkS))
  (fp_text value TO-220AB_STM (at 2.54 -0.65 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 2.54 -0.65 unlocked) (layer F.Fab))
  (pad "1" thru_hole rect (at 0 0) (size 1.651 1.651) (drill 1.143) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at 2.54 0) (size 1.651 1.651) (drill 1.143) (layers *.Cu *.Mask))
  (pad "3" thru_hole circle (at 5.08 0) (size 1.651 1.651) (drill 1.143) (layers *.Cu *.Mask))
)
