(module TO-220F-5_P3.4x2.06mm_StaggerEven_Lead1.86mm_Vertical (layer F.Cu) (tedit 5AF05A31)
  (descr "TO-220F-5, Vertical, RM 1.7mm, PentawattF-, MultiwattF-5, staggered type-2")
  (tags "TO-220F-5 Vertical RM 1.7mm PentawattF- MultiwattF-5 staggered type-2")
  (fp_text reference REF** (at 3.4 -5.62) (layer F.SilkS))
  (fp_text value TO-220F-5_P3.4x2.06mm_StaggerEven_Lead1.86mm_Vertical (at 3.4 4.21) (layer F.Fab))
  (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 1.7 2.06) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 3.4 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 5.1 2.06) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 6.8 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask))
  (fp_text user %R (at 3.4 -5.62) (layer F.Fab))
  (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220F-5_P3.4x2.06mm_StaggerEven_Lead1.86mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)