(footprint "TO-92_Inline" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5A1DD157)
  (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
  (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
  (attr through_hole)
  (fp_text reference "REF**" (at 1.27 -3.56) (layer "F.SilkS"))
  (fp_text value "TO-92_Inline" (at 1.27 2.79) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab"))
  (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask))
  (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask))
  (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask))
  (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
