(module TP4056 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value SOP8-PP_TPW (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.05in/1.27mm" (at -5.76935 -1.27) (layer Cmts.User))
  (fp_text user "0.022in/0.558mm" (at 5.76935 -1.905) (layer Cmts.User))
  (fp_text user "0.214in/5.443mm" (at 0 -4.9657) (layer Cmts.User))
  (fp_text user "0.057in/1.455mm" (at -2.72135 4.9657) (layer Cmts.User))
  (fp_text user "0.134in/3.404mm" (at 7.5819 0) (layer Cmts.User))
  (fp_text user "0.099in/2.515mm" (at 0 6.2357) (layer Cmts.User))
  (fp_text user "*" (at -2.97535 -3.606) (layer F.SilkS))
  (fp_text user "*" (at -1.6129 -2.4765) (layer F.Fab))
  (pad 1 smd rect (at -2.721348 -1.905) (size 1.454899 0.558) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.721348 -0.635) (size 1.454899 0.558) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.721348 0.635) (size 1.454899 0.558) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.721348 1.905) (size 1.454899 0.558) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 2.721348 1.905) (size 1.454899 0.558) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2.721348 0.635) (size 1.454899 0.558) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 2.721348 -0.635) (size 1.454899 0.558) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 2.721348 -1.905) (size 1.454899 0.558) (layers F.Cu F.Paste F.Mask))
  (pad EPAD smd rect (at 0 0) (size 2.5146 3.4036) (layers F.Cu F.Paste F.Mask))
)
