(module TPS74633PQWDRBRQ1 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value WSON_PQWDRBRQ1_TEX (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.026in/0.65mm" (at -4.4934 -0.649986) (layer Cmts.User))
  (fp_text user "0.012in/0.306mm" (at 4.4934 -0.974979) (layer Cmts.User))
  (fp_text user "0.114in/2.891mm" (at 0 -3.9624) (layer Cmts.User))
  (fp_text user "0.032in/0.808mm" (at -1.4454 3.3274) (layer Cmts.User))
  (fp_text user "0.098in/2.489mm" (at 3.9624 0) (layer Cmts.User))
  (fp_text user "0.069in/1.753mm" (at 0 4.5974) (layer Cmts.User))
  (pad 1 smd rect (at -1.4454 -0.974979) (size 0.807999 0.3056) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.4454 -0.324993) (size 0.807999 0.3056) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.4454 0.324993) (size 0.807999 0.3056) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.4454 0.974979) (size 0.807999 0.3056) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.4454 0.974979) (size 0.807999 0.3056) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.4454 0.324993) (size 0.807999 0.3056) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.4454 -0.324993) (size 0.807999 0.3056) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.4454 -0.974979) (size 0.807999 0.3056) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0 0) (size 1.7526 2.4892) (layers F.Cu F.Paste F.Mask))
)
