(module TPS76901QDBVRG4Q1 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value DBV5 (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at -1.4478 -2.6518) (layer F.Fab))
  (fp_text user "*" (at -1.4478 -2.6518) (layer F.SilkS))
  (pad 1 smd rect (at -1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.1938 0) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask))
)
