(footprint "TQFP-64_14x14mm_P0.8mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "64-Lead Plastic Thin Quad Flatpack (PF) - 14x14x1 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
	(tags "QFP 0.8")
	(property "Reference" "REF**"
		(at 0 -9.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "TQFP-64_14x14mm_P0.8mm"
		(at 0 9.45 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -7.7 -6)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "2" smd rect
		(at -7.7 -5.2)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at -7.7 -4.4)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "4" smd rect
		(at -7.7 -3.6)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "5" smd rect
		(at -7.7 -2.8)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "6" smd rect
		(at -7.7 -2)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "7" smd rect
		(at -7.7 -1.2)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "8" smd rect
		(at -7.7 -0.4)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "9" smd rect
		(at -7.7 0.4)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "10" smd rect
		(at -7.7 1.2)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "11" smd rect
		(at -7.7 2)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "12" smd rect
		(at -7.7 2.8)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "13" smd rect
		(at -7.7 3.6)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "14" smd rect
		(at -7.7 4.4)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "15" smd rect
		(at -7.7 5.2)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "16" smd rect
		(at -7.7 6)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "17" smd rect
		(at -6 7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "18" smd rect
		(at -5.2 7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "19" smd rect
		(at -4.4 7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "20" smd rect
		(at -3.6 7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "21" smd rect
		(at -2.8 7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "22" smd rect
		(at -2 7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "23" smd rect
		(at -1.2 7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "24" smd rect
		(at -0.4 7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "25" smd rect
		(at 0.4 7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "26" smd rect
		(at 1.2 7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "27" smd rect
		(at 2 7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "28" smd rect
		(at 2.8 7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "29" smd rect
		(at 3.6 7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "30" smd rect
		(at 4.4 7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "31" smd rect
		(at 5.2 7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "32" smd rect
		(at 6 7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "33" smd rect
		(at 7.7 6)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "34" smd rect
		(at 7.7 5.2)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "35" smd rect
		(at 7.7 4.4)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "36" smd rect
		(at 7.7 3.6)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "37" smd rect
		(at 7.7 2.8)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "38" smd rect
		(at 7.7 2)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "39" smd rect
		(at 7.7 1.2)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "40" smd rect
		(at 7.7 0.4)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "41" smd rect
		(at 7.7 -0.4)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "42" smd rect
		(at 7.7 -1.2)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "43" smd rect
		(at 7.7 -2)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "44" smd rect
		(at 7.7 -2.8)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "45" smd rect
		(at 7.7 -3.6)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "46" smd rect
		(at 7.7 -4.4)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "47" smd rect
		(at 7.7 -5.2)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "48" smd rect
		(at 7.7 -6)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "49" smd rect
		(at 6 -7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "50" smd rect
		(at 5.2 -7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "51" smd rect
		(at 4.4 -7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "52" smd rect
		(at 3.6 -7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "53" smd rect
		(at 2.8 -7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "54" smd rect
		(at 2 -7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "55" smd rect
		(at 1.2 -7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "56" smd rect
		(at 0.4 -7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "57" smd rect
		(at -0.4 -7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "58" smd rect
		(at -1.2 -7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "59" smd rect
		(at -2 -7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "60" smd rect
		(at -2.8 -7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "61" smd rect
		(at -3.6 -7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "62" smd rect
		(at -4.4 -7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "63" smd rect
		(at -5.2 -7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "64" smd rect
		(at -6 -7.7 90)
		(size 1.5 0.55)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-64_14x14mm_P0.8mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)