(module TS5USBA224RSWR (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value RSW10 (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at -1.735024 -0.781) (layer F.SilkS))
  (fp_text user "*" (at -1.735024 -0.781) (layer F.Fab))
  (pad 1 thru_hole rect (at -0.649224 -0.2 90) (size 0.2 0.9) (drill 0.762) (layers *.Cu *.Mask))
  (pad 2 smd rect (at -0.700024 0.2 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.399999 0.900049) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0 0.900049) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0.399999 0.900049) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.700024 0.2 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.700024 -0.2 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0.399999 -0.900049) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0 -0.900049) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -0.399999 -0.900049) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask))
)
