(footprint "TSNP-16-9" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "U**" (at 0 -2.1 unlocked) (layer "F.SilkS"))
  (fp_text value "TSNP-16-9" (at 0 2.2 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0 3.7 unlocked) (layer "F.Fab"))
  (pad "1" smd roundrect (at -1 1.05) (size 0.25 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
  (pad "2" smd roundrect (at -0.5 1.05) (size 0.25 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
  (pad "3" smd roundrect (at 0 1.05) (size 0.25 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
  (pad "4" smd roundrect (at 0.5 1.05) (size 0.25 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
  (pad "5" smd roundrect (at 1 1.05) (size 0.25 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
  (pad "6" smd roundrect (at 1.05 0.5) (size 0.25 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
  (pad "7" smd roundrect (at 1.05 0) (size 0.25 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
  (pad "8" smd roundrect (at 1.05 -0.5) (size 0.25 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
  (pad "9" smd roundrect (at 1 -1.05) (size 0.25 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
  (pad "10" smd roundrect (at 0.5 -1.05) (size 0.25 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
  (pad "11" smd roundrect (at 0 -1.05) (size 0.25 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
  (pad "12" smd roundrect (at -0.5 -1.05) (size 0.25 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
  (pad "13" smd roundrect (at -1 -1.05) (size 0.25 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
  (pad "14" smd roundrect (at -1.05 -0.5) (size 0.25 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
  (pad "15" smd roundrect (at -1.05 0) (size 0.25 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
  (pad "16" smd roundrect (at -1.05 0.5) (size 0.25 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
  (pad "17" smd roundrect (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.03333333333)
    (thermal_bridge_angle 45))
)
