(footprint "TSOT-23-5" (version 20240108) (generator "pcbnew") (generator_version "8.0")
  (layer "F.Cu")
  (descr "TSOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "TSOT TO_SOT_SMD")
  (property "Reference" "U1" (at -0.6 -1.5 0) (layer "F.SilkS")(hide yes))
  (property "Value" "3V3. 500mA" (at 0 2.4 0) (layer "F.Fab"))
  (property "Footprint" "" (at 0 0 0) (layer "F.Fab")(hide yes))
  (property "Datasheet" "" (at 0 0 0) (layer "F.Fab")(hide yes))
  (property "Description" "" (at 0 0 0) (layer "F.Fab")(hide yes))
  (property "Digikey" "" (at 0 0 0) (layer "F.Fab")(hide yes))
  (property "LCSC" "C587158" (at 0 0 0) (layer "F.Fab")(hide yes))
  (property "Part" "TPRT9013-33GB" (at 0 0 0) (layer "F.Fab")(hide yes))
  (attr smd)
  (fp_text user "${REFERENCE}" (at 0 0 0) (layer "F.Fab"))
  (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-5.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
